Hearing Aid Compatibility Information

A list of all devices offered by Choptank Fiber, including hearing aid-compatibility ratings and FCC IDs can be found here: (Insert link to excel sheet)

Devices showing an M/T rating are evaluated under the ANSI 2011 Standards. Devices showing Hearing Aid Compatible are evaluated under the current 2019 ANSI standards.

For more information on ratings and ANSI standards visit: <https://www.fcc.gov/hearing-aid-compatibility-wireless-telephones>

The rating system is explained by the FCC as: “The “M” rating is for reducing interference with hearing aids operating in acoustic mode—from M1 to M4, with M4 being the best. The “T” rating is for their ability to operate with hearing aids that contain a telecoil (a tightly wrapped piece of wire that converts sounds into electromagnetic signals) and operate in inductive coupling mode—from T1 to T4, with T4 being the best. The FCC considers a handset to be hearing aid-compatible if it is rated at least an M3 (for acoustic coupling) and at least a T3 (for inductive coupling).”

All devices are compatible under 2011 ANSI standards. Only devices shown as “Hearing Aid Compatible” are compatible under the 2019 ANSI standards.

For more information about the wireless hearing aid compatibility rules and service providers' obligations visit: <https://www.fcc.gov/hearing-aid-compatibility-wireless-telephones>

For more information regarding hearing aid-compatible and non-hearing aid-compatible handset models visit: <https://www.gari.info/>